**CHURNING MACHINES**

25L 37L 40L 55L

**USER MANUAL**

Dear Customers;

First of all, thank you for purchasing our product.

This guide from quality control before you can use your machine to have passed in the most efficient way has been prepared for the purpose. Therefore, this guide is right on, we advise you to read carefully before using the product, and we advise you to keep a reference to the source.

**TABLE OF CONTENTS**

Churning machinery and technical characteristics

Presentation of the product

Packing and Transport Information

Installation and Connection

Safety Instructions

Operating instructions

Cleaning and maintenance

Churning Machine Hygiene Rules

Troubleshooting

Churning Machine Spare Parts List



**PRESENTATION OF THE PRODUCT**

* This product is used to obtain the butter from the yogurt
* Very easy Assembly and disassembly-clean the propeller system » Stainless steel body
* New powerful engine
* Quality Chuming Machine
* Perfect appearance
* Ergonomic use
* Easy control panel

**PACKAGING AND TRANSPORT INFORMATION**

* Each carton contains one Churning.
* Shipping container and do not tilt the product side.
* Shipping container and place súrimeyiniz.
* The maximum number of consecutive 4 duct can be put.
* Product when not in use for a long period of time, orif not sold, dry, free of dust and humidity should be stored in an environment without.

**INSTALLATION AND CONNECTION**


* There is no need to link to a special water.
* You can dump the water into the boiler using the hose.

**SAFETY INSTRUCTIONS**

* Your product is put into the ground in accordance with local and national instructions.
* Use only on a flat surface in your product.
* The power cord is damaged, to avoid any danger, so that only authorized company or must be replaced by an authorized service.
* Avoid moving the product while machine is running.
* This product is children, the elderly, the disabled does not provide complete protection for.
* The main voltage ¡is the voltage at the same product make sure the specified in the tag.
* Do not use the product for other matches.
* Plug must be appropriate. The outlet must not move in.
* This product should be used entirely appropriate national standards; Please follow all the instructions to use.
* Product with a cable and plug or another ¡is allowed with the tool from within in order to ensure that the wire cables, insulation thickness of at least 3 mm in all Poles must be that this insulation is essential to be provided with fixed wire, too.
* Product is allowed with a cable and plug the cable that needs to be available in the product.
* The product must be used in a completely flat floor and must be kept away from flammable material.
* Product kablosonu can cut or damage wire in place, cover, and do not hold closely to the hole. The power cord is damaged, to avoid any danger, so that only authorized company or must be replaced by an authorized service.

**OPERATING INSTRUCTIONS**.

* Authorized company arising from the use of the product in question for other purposes cannot be held responsible for malfunctions or damage.
* Before you begin using the product Use, please read through the Manual carefully. Thus, both yourself and you can protect your product from possible damage.
* Use the product in accordance with the instructions for use. Thus, in the case of electrical Assembly products to contact home.
* Churn churn using the machine in accordance with the label using the time and note the amount of yogurt.
* Unplug this product from the power into the main socket. e Run from the switch to the machine.
* When you start to put yogurt in a bucket bucket do not pass the level indicator.



* Keep away from children and churning Machine.
* Do not use your machine on a carpet, do not close the pores at the bottom of the machine.
* After each operation, rinse with plenty of hot water in the product.

**CLEANING AND MAINTENANCE**

* Unplug the product from the electrical outlet after each use, remove.
* The machine, wipe it with a cloth slightly damp.
* After cleaning with a damp cloth, wipe the product with a dry cloth ¡is definitely.
* Equipment for cleaning do not use steam or pressure cleaning materials.
* Do not use chemical cleaning agents or steel.
* lfthereis a problem with your product, turn off the power button from your product. Unplug it plug out and call the Authorized Service. Product is fully repaired, the electricity do not link with.

**CHURNING MACHINE HYGIENE RULES**

* Yogurt and Ayran churn do not leave inside the machine for six hours. » Clean with hot water after using the product, 80c-100c
* Remove and clean the propeller after each use.
* Make sure cleaning the hose.

**PROBLEM-SOLVING**





**CHURNING MACHINE SPARE PARTS LIST**

40L / 55L Cr.Ni. Round Win

Switch Condenser

Condenser Slot (single)

Condenser Slot Screw

40L/55L the lower Circle Round

40L/55L top cover Round

Top Cover Handle

Top Cover Screw

Propeller

Complete Hub

Complete Churning Engine

Churning Hub Pulley

Churning Engine Shaft Pulley

V Spin

Cable Wrap Arm

Drain Hose

Drain Hose Clamp

Plug and Cable

Hose Hanger

Machine base (unit)

Machine base Screw