**Instructiong Manual**

**Electric potato chip machine**

****

 **Please read the introduction before using**

**IMPORTANT SAFEGUARDS:**

**When using this potato chip machine, basic safety precautions should always be**

**followed including the following**

1.Read all instructions.

2.To Protect against risk of electrical shock do not put in water or other liquid

3. Unplug from outlet when not in use, before putting on or taking off partes, and before cleaning.

4.Avoid contacting moving parts

5. Do not operate any appliance with a damaged cord or plug or after the machine

malfunctions, or is dropped or damaged in any manner. Return the machine to the nearest

authorized servo is facility for examination, repair or electrical or mechanical adjustmeln

6. Do not use outdoors

7. Do not let cord hang over edge of table or counter

8. Do not let cord contact bot surface, including the stove

9. Do not touch the moving parts when in operation

10. Blade is sharp. Handle carefully

11. If the power cord is damaged, it must be replaced by the service agent or a similarly

qualified person in order to avoid hazard

12. This machine is not intended for use by person(including children )with reduced physical

sensory or mental capabilities, or lack of experience and knowledge, unless they have

been given supervision of ins ruction concerning use of the appliance by a person

responsible for their safety

13. Children should be supervised to ensure that they do no play with the appliance

14.Care is needed when handing cutting blade during cleaning

**SAVE THESE INSTRUCTIONS**

**Specificaion:**

**110V,220V,40W**

**Description:**

1. Main body: full 201#stainless steel material

2. Control penal (with the buttons of "ON/OFF), the button is inching switch

3. Potato holde, three sets blade&mould Size for potato chip is:

6mm. 9mm 13mm

**How to use:**

1. plug in the machine to the power

2. Press the"NO/OFF"button, When press it, the pressing mould will

move, when stop pressing the button, it will stop mocing

3. lsert the potato into the potato holder, then press the NO/OFF button, keep on

pressing the button, unill the potato si finished cutting

4. Press the button to another side the pressing mould will life up, ther can repeat No

3 to begin another cycle

5. About changing the blade mould: If you need another size s potato chip, then adjust

the screws of the blade set and the black mould take out the blade and the black

mould, install another size blade &black mould

6. Cleaning:

Unplug the machine

clean the chamber with wet cloth. Do not clean hte blade by hand

Remove the blade from the machine for cleaning if necessary.