**1. Purpose and the working eprinciple**

This machine professional use for separate the shell and the seeds ,such as :the almond ,the a walnut .

**2. The structure and capability**

The dimension : 2100\*800\*1550mm

This machine make by :the feeding ,the shaking ,the fan and other parts .

We use the rubber bearing ,this is better for use .This machine is use to control the size for wind come in and the anqule of the shaking machine to get a good depart of the shell and the seeds.

**3. The operation of this machine**

(1) Before use this machine should check whether the machine is good in the

transportation .

(2) In the working system ,the seeds and the shell should full on the shaker screen ,so that can get a good quality .

(3) If the separate is not good ,please change the anqle of the shaking mahcine or ,the wind inside part.

**4. The maintenance**

(1) Before running the machine ,should check the screws first .

(2) Add the lubricant oil on the bearing on time .

(3) Should check the rubber belt after working sometime.

Model: SF-300

Capacity: 600 kg/h   
Power: 3 KW, three phase 380V

****