**Operation Steps of Crushing Machine**

1. **Install the belt,remove the belt protective cover,install the crusher belt and adjust the tightness of crusher belt(the belt can be pressed down 1-2CM with finger),install the belt protective cover,check every connection parts to make sure whether it is firm and reliable or not.**
2. **Close the feed valve,add the material into the feed hopper,tie the cloth bag well.**
3. **Start the machine and make the machine idle for 2-3 minutes,observe whether there is abnormal situation or not.**
4. **Slowly open the feed valve to 1/3 position(according to the material situation and motor load conditions to adjust appropriately the valve opening degree,so as not to overload the motor)**
5. **After processing all materials,idle the machine for 1-2 minutes,close the power switch after all the material is completely eliminated.**