**Hay cutter**

**Functions and features:**

1. Steel frame, small size, light weight, easy to move  
2.Safety device designed to stop eating knife accidents, safe and reliable machine.  
3. Grass roller shaft universal coupling, compact structure, flexible operation, easy disassembly  
4. Supporting dynamic and diverse selection, motors, diesel engines, tractors can be complementary, especially in areas lacking electricity more appropriate.  
5. Blade made of high quality steel, with a special refining process, super wear; using high strength bolts, safety and reliability.  
6. Continuous use thicker steel chassis welded overall mold forming, pressing counterfeit trademark, beautiful and durable.  
7. Excellent value for money, chaff lowest price equal productivity.

|  |  |
| --- | --- |
| **Model No** |  |
| **Dimension(L\*W\*H)mm** | **850\*420\*810** |
| **Packing size(L\*W\*H)mm** | **530\*400\*300** |
| **Rated power** | **2.2kw** |
| **Rated voltage** | **220v** |
| **Rated motor speed** | **2800r/min** |
| **net weight** | **41kg (without electric motor)** |
| **Productivity** | **>600kg/h** |
| **Finished length** | **3-5cm** |
| **Spindle speed** | **800rpm** |

